Individually Floating Rechargeable Electric Shaver
	[image: electric shaver]
	[image: black shaver]

	[image: men shaver]
	[image: two color shaver]


 ABIS Mold was found in 1996 in Shenzhen, adjacent to HK, China. and we moved to Long gang District in 2010.With the advanced facilities from Germany, Switzerland and Japan, and a highly experienced design and engineering team. Our molding press machine ranges from 40T to 650T, 300+ molds capacity each year, and 70 % are exported to Europe and North America.        [image: IMG_260]
  In addition to our plastic mold and molding specialties, we also can provide you the services such us die casting, stamping /punching, blowing mold, as well as the secondary process.

Product Description
	Part Name
	​Individually Floating Rechargeable Electric Shaver 

	Description                                  
	Man Shaver

	Country of Original
	China (ShenZhen)

	Current Export Markets
	North America

	Lead Time
	30 Days



Key Specification 
Pop-up trimmer
With On/Off switch
3-head rechargeable shaver
Comfortable and perfect shaving
Triple heads individually floating
Cord charge with charging indicator
Accessories: Cleaning brush and charging cord
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Project Procedure
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Payment Terms
 1. T/T: 40% Deposit,30% upon T1 Sample,30% Balance before shipment
 2. L/C: irrevocable 100% L/C at sight.
Workshop
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Certification
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Tooling Shop
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QC Control
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Packaging & Delivery
Packaging Details：Free-Fumigation Three-Plywood case
Delivery Detail: 25-35 days by sea, 3-7 days by air
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	ABIS MOLD TECHNOLOGY CO.,LTD
Daisy Wang (Overseas sales)
Web: www.abismold.com
Cell/whatsapp: +86-15016526799
Skype: daisymold@outlook.com
Email: Daisy@abismold.com
Add: Building B#,YingKeli Industrial Part, LongDong Community, 
    LongGang District, Shenzhen, China 518116



FAQ

 Q: What can we do if we don't have the mold drawing?
 A: you will only provide the actual sample to us then we can help you to make the design injection  mold drawings for your confirmation.
 
 Q: Can we test the plastic injection mold?
 A: After the mold is ok ,we can help you to test the mold for free.
 
 Q: What can you do for you?
 A: Make optimum solution to reduce your cost
 B: Product your idea and design to products
 C: Quality inspection and inspection report
 D: Professional export service 

 Q: Before shipment, how to make sure the products quality?
 A: If you don't come to our factory and also don't have the third party for inspection, we will be as your 
 inspection worker. We will supply you a video for production process detail include process report, 
 products size, structure and surface detail, packing detail and so on.
 
 Q: Can you do post production?
 A: Some customers in addition to plastic injection require post processing, assembly of their products 
 and packaging. 
   
 Q: Is it possible to know how are my products going on without visiting your company?
 A: We will offer a detailed production schedule and send weekly reports with digital pictures and videos 
 which show the machining progress.
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Mold Making QC main steps

Plastic Molding QC main steps

'Mould Design Control : Design review checkist before
submitting to the customer. We will not start the steel

‘purchasing work until get your written approval on our mold

drawing.

Incoming quality control: all steel material and outsourcing
standard components will be checked to ensure that they are
in accordance with the BOM(QTY and material/components

‘name specified).

In process quality control: all the machining and assembling

process is under control, we have C team to check and

supervise the tolerance and processed surface to satisfy the

requirements. (Mould Steel Hardness Inspection, Mould

Electrodes Inspection, Mould Core and Cavity Steel Dimension

Inspection , Mould Pre-Assembly Inspection )

Final quality control: within 3 days the completion of the

plastic mold, we will have a thorough check for the main size:

of the molded plastic sample and mold to ensure that the
critical o full dimension (if required) are within tolerance.

Mould Pre-Shipment Final Inspection : Free-fumigation three-
plywood case packing; make sure the mold is conformity to the

‘approved mold drawing. The spare components and easily
broken components and the electrode (if required) are

packaged, as well as the mold drawing and some certificated.

Vernier caliper measurement is performed by our
trained operators when the first product comes out of
‘our machine, we check the contour dimensions and
‘assembly status (if exist) to identify if any rejects.

The molded parts are then inspected again by our
experienced QA department for the full dimensions
especially the critical dimensions set by customer, and
quality result was recorded at the same time. The
Result will be to our QC Supervisor directly to see if the
unqualified dimensions (if exist) are caused by the
uncontrolled factors or our mistakes and we will take
the related actions to improve t.

‘We will rustily report the T1 result to customers, and.
send T1 samples to customers for checking -
Sometimes T1 samples need improvements, If good
samples are required by customer at first, we will take
actions to improve the mold to make sure the samples
have 0 defects. No shrinkage, warpage, flash, material
streak, air bubble, step line, ejector mark, and
dimension within tolerance.

Package inspection: make sure QTY/color (if required)
and weight are correct.
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